IC-2340H 
X-BAND REPEATER 

1- Set desidered Freq. on each band 2- Press "VHF" and "UHF main" and " SET" at the same time. 
(Memmory indicator will change to "L". EXIT - Press "SET" for 1 second.