To put the 731A into crossband...
Press the F key and then press the A.B.C. key. Three dots should be lit in both display frequencies. The unit will now operate as a cross band repeater 

To take the 731A out of crossband...
Press the F key and then press the A.B.C. key. 
The three dots should go out in both display frequencies. The unit will now operate normally